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Close Coupled Back to Wall Toilet Suites

DESCRIPTION 
• Rimless, hygienic flush pan
• UF quick release, soft close seat
• High quality, R&T flush mechanism
• Water inlet: top left or bottom right inlet;
• Included components: 
Toilet tank 4.5/3L
Toilet Pan, P Trap
UF cover&seat
Vario pan connector for Strap
Fill valve
• [image: ][image: ]S-Trap Installation: set out: 70-140mm
• P-Trap installation: set out: 180mm   
                                        

                                                                          Standard Installation
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