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Anti-bacterial glazing
Super hydrophilic
Anti-stain technology
Easier cleaning 
            Rimless technology  














	
· Code: AB2232+AS8232D
· Warranty:  25 Years warranty on ceramic  
                            1 Years warranty on the toilet seat 
                            3 Years warranty on the cisterns valves， plastic and internal parts 





Specifications
[bookmark: OLE_LINK1][bookmark: _Hlk120470243]AB2232H+AS8232D 
[bookmark: _GoBack]Close Coupled Back to Wall Toilet Suite
[image: 图片包含 杯子, 黑暗, 桌子, 玻璃

描述已自动生成]
Soft close, quick release seat
WELS 4 star, 4.5/3 ltrs/min
[image: 徽标

中度可信度描述已自动生成]Size: 654X398X810MM
  Bottom and back inlet available
• S-Trap Installation: set out: 70-140mm
• P-Trap installation: set out: 185mm        

                                                                                                                                
                                                                                                                                       

                    
                      Model AB2232H+AS8232D                                                   Standard Installation                                 
                                                    Toilet outlet
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140mm Recommended
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